{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["scenario 1","scenario 2","case study"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"scenario 1","index":0,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["TWSC Intersection Model (Scenario 1) - Computational Engine"]
[]
["Given Conditions","EBTH","NBTH"]
["Movement",2,8]
["Volume",600,100]
["tc",null,4.0999999999999996]
["tf",null,2.2000000000000002]
[]
["Calculations","EBTH","NBTH"]
["Conflicting flow, vc",null,{"$f":"B5","v":600}]
["Capacity, c",null,{"$f":"PotCap(C10,C6,C7)","v":986.96657638691067}]

{"sheet":"scenario 2","index":1,"n_rows":14,"n_cols":4,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["TWSC Intersection Model (Scenario 2) - Computational Engine"]
[]
["Given Conditions","EBTH","WBLT","NBLT"]
["Movement",2,4,7]
["Rank",1,2,3]
["Volume",600,100,50]
["tc",null,4.0999999999999996,7.1]
["tf",null,2.2000000000000002,3.5]
[]
["Calculations","EBTH","WBLT","NBLT"]
["Conflicting flow, vc",null,{"$f":"B6","v":600},{"$f":"B6+2*C6","v":800}]
["Potential capacity, cp",null,{"$f":"PotCap(C11,C7,C8)","v":986.96657638691067},{"$f":"PotCap(D11,D7,D8)","v":305.50231776737098}]
["Impedance factor",null,null,{"$f":"1-C6/C12","v":0.8986794463029536}]
["Movement capacity, cm",null,null,{"$f":"D12*D13","v":274.54865377544996}]

{"sheet":"case study","index":2,"n_rows":19,"n_cols":4,"rows_kept":19,"cut":false,"hidden":false,"merged":[[18,1,18,3]]}
["TWSC Intersection Model (Case Study) - Computational Engine"]
[]
["Given Conditions","NBTH","SBLT","EBLT"]
["Movement",2,4,7]
["Rank",1,2,3]
["Volume",450,300,100]
["tc",null,4.0999999999999996,7.1]
["tf",null,2.2000000000000002,3.5]
[]
["Calculations","EBTH","WBLT","NBLT"]
["Conflicting flow, vc",null,{"$f":"B6","v":450},{"$f":"B6+2*C6","v":1050}]
["Potential capacity, cp",null,{"$f":"PotCap(C11,C7,C8)","v":1121.1191493206668},{"$f":"PotCap(D11,D7,D8)","v":206.94635049914999}]
["Impedance factor",null,null,{"$f":"1-C6/C12","v":0.73241024365538432}]
["Movement capacity, cm",null,null,{"$f":"D12*D13","v":151.56962699267501}]
[]
["Performance measures","EBTH","WBLT","NBLT"]
["Movement v/c ratio",null,{"$f":"C6/C12","v":0.26758975634461563},{"$f":"D6/D14","v":0.65976279010591454}]
["Movement delay",0,{"$f":"TWSCDelay(C6,C12)","v":9.3801136205179478},{"$f":"TWSCDelay(D6,D14)","v":65.829365665244097}]
["Intersection delay",{"$f":"(B18*B6+C18*C6+D18*D6)/SUM(B6:D6)","v":11.055259591387994}]